Function tree:

Working of machine

Lifts the load from the location

Machine unloads at required location

Machine receives command an process it

Unloading starts

If not appropriate it rejects by indicating it with red light

If it is appropriate load it

Checks the weight limit

Machine starts loading

Turn on/off

Receive and process speed adjustments

Machine gets on

Choose speed adjustments(1,2,3)

Receive and process command

Unloading

Loading

Receiving commands